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1.0
Refreshing  subsystem

Log into Replication Manager (you will need replication manager permissions from within DeviceManager)
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Select ‘Subsystem’ screen under ‘Resources’ Pane.

Check all the Subsystems you require HRpM to scan for configuration updates.
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Execute the Refresh by clicking on [Refresh Subsystem] button

1.1
Determining Journal group 
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From HRpM  ‘Subsystems’  screen ,  select the primary subsystem.

Then select the ‘JNLGs’ pane. This will take you into the JNLGs window
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From the  above  ‘JNLGs’ screen, note the next available Journaling group for  later use in creating your  HUR replication  pairing group

1.3
Setting up ‘My Copy Groups’ in HRpM
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From the  HRpM screen

Click on the [My Copy Groups] Panel

On  the My Copy Groups screen . click on [Edit My Copy Groups] button  the ‘Edit my copy groups’  dialog screen will pop-up
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Check the Copy Groups you wish to manage 

Then click on [ok] button to revert to the ‘My Copy Groups’ screen

2.0 
Setting up  Replication (HUR)
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From HRpM ‘Resources->Hosts’ select   The host for Replication.

Click on the  ‘Unpaired ‘ Tab 
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Select the Primary  volumes (P-Vols ) from the  ‘Unpaired’ panel.

Click on [Pair Management] to launch the HRpM Pair Management Wizard

[image: image9.emf]
On the ‘Pair Association”  screen above,

Click on [Add Group] to add new pair group for the selected  P-Vols .  This will bring up a ‘Add Pair Group’  dialog that will allow you to create  a new group into the topology at the top of the screen.

[image: image10.emf]
Enter a name for the new  pair group  following the recommended standards  (e.g  UR pairing <hostname>_<serailnum P-VOL array>_<serailnum S-VOL array>_<2 digit Journal group>)

Select the copy Type for the new pair group. (eg UR for UR Replication or SI for PIT copy)

Click the [OK] button to proceed
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The newly created pair group is shown on the upper copy topology pane
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On the Right –below  pane under  ‘Volume Selection’ ,start selecting the target remote volumes S-VOLs . Specify the filter conditions : Site (FDC or RDC), 

Host Name (Leave Blank), 

Subsystem ( Select remote ip & serial number)

Logical Group  . Click on the [Refresh ] button to start searching the voulmes that match the filter conditions.

Select the Target volumes from the ‘Candidate’ list box

Click on [<Add Selection] button to add  selected volumes  as S-VOLs.
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Confirm the ‘Pair list’  listing for P=VOl and S-VOl association  is correct  and  click the [next] button
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On the ‘Group Management’ screen above 

Select the pair group that you want the copy group to be created. You will notice that the selected pair group is not assigned to any copy group.

Click on [Create Group] button to create a copy group for the select ed pair group. This will pop up  a  ‘Create group’ dialog that will allow you to specify the pair managmenet servers and HORCM related parameters.
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On the ‘Create Group’ screen above

Confirm the Group Name has  the Coyp Group name entered earlier

Confirm the Primary and Secondary Pair Management server name .

Specify the HORCM instance  number to create this copy Group ( Use the standards detailed in the check sheet 0 -> primary  and 1 -> secondary  3 ->ShadowImage   primary  4-> ShadowImage   secondary)

As these are already defined you will only need to select them from the drop down list.

Click on [OK] button to proceed to create Copy Group
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On the ‘Group Management’ screen above.

The newly created copy group is shown on the left pane.

Click on [<Apply] button to add the copy pairs shown in the  ‘Pair  list’ Listing pane.
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On the ’Group Management’ screen above,

The Copy Pairs have been assigned to the newly created copy group.

Click on [Next>] button to proceed to set the task execution options for  pair creation (copy pace, fence level, journal group, etc)
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On the ‘Task Management’ screen above , the list  of the tasks is displayed . One task  corresponds to one Copy Group.

Click on the Task icon. This will pop-up a task Dialog box .This will allow you to edit the execution schedule and copy pair settings for the pair creation.
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  From the ‘Edit Task’ Pane

Click on the’ Pair Setting’ Panel
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For HUR Confirm the ‘Copy Pace’   is set to 15 and the Fence is set to ‘ Async’
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Modify the ’Journal ID (p)’ and ’Journal ID (s)’ to be the same as determined in the tracking sheet

Click on  [OK]  button to save the settings and proceed to the  Pair Configuration confirmation screen
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On the ‘Task Management’ Screen now click [Next>] button to proceed to  the confirm window.

[image: image23.png]p 001dr:23016 - Pair Configuration Wizard - Microsol plo =] E3

1. Intraduction b 2. Pair Assaciation b 3. Group Management b 4. Task Management b 5. Confirm b 6. Finish

Check the sattings for copy pair configuration,
Carsfully raview the summary balow, and then dick "Confirm" o 3pply all the changes
This oparation might take several minutes to finish,

Copy Topology |

H— &

uR

Pair List |

Copy Types  Copy Group Name Pair Name POrt/HSD/LUN Subsystem Capacity Logical Group Label
) CLL-C/fdegegad00indip Ipfeo/02  USP_V@L0.159.28.107 (18779) 34,6968 fdcgegadodinolp2p  Replication ol
w fdegeaadddindip 1677918950 03 P_6004:6004.007 ¢y Chrdcgegadoninginz UsP_v@165.186.192.144 (18850) 54169 6B rdcgegadoningicnoze | Replication Wols
) CLi-C/fdcacgad001n01p Ipfeo/03  USPV@10.159.28.107 (18779) 34,6968 fdcgegado0inoip-2p  Replication ol
m fdegegadddindilp 167791885003 600560050072 ¢y Cridcgeadnningiens UsP_v@165.186.192.144 (18850) 34169.GB  rdcgegadoninicnoze  Replication Wols

Copy Group List

CEloe e Pair Configuration File(Primary) Pair Configuration File(Secondary)
Name Type Server Name File Instance Port Server Name File Instance Port
fdcgegadooingip_18779_18850_03 R fdesan-matL.eurnsroot.net horemo.conf 0 5300 rdesan-mgtt.eurnsrostnet horem. conf 1 sm

[

Trusted sites

Eoone [
istert| [ (@ @ | &) interet ExplorerEnhan.. | £ Htach Device Manager .| ] htpsifitctisvhmontars. .. | 1 itach Device Manager .. | &) ntpssifctisvhmonter:... [ hecpss//Mecisvhamoo.. | @ 28w





[image: image24.png]Copy Group List

CEloe e Pair Configuration File(Primary) Pair Configuration File(Secondary)

Name Type Server Name File Instance Port Server Name File Instance Port

fdcacaado01n0lp 167751885003 UR fdcsan-matt.eunnsrotinet  horcmo.conf 0 330 rdcsanmatlewnnsootnet  horemi.cont 1 s

Task List |
Tioo =1 | i) [i|pagei of1 (11l 1

Copy Group & copy Type Pairs | Pairs Operations Execution Request Time

fdcgegadoninolp_1773_16850_03 s 2 modify fle + creste Immediately

<. T have. sanfirmed the. abave infarmatian and wish a creats pair sanfiauration
(<nari) [ eomemn ] aneal) (riin) LT

Eiooe [l e ses
istort| [ (@ @ | &) intere ExplorerEnhan.. | ] Htach Device Menager .| ] htpsifitctisvhmniars. .| €1 itach Device Manager .. | &) tpssifctsvhmonter:... [ hetpss//Mectisvhanoo. | @ 28w





On the ‘Pair Configuration->Confirm’ screens above

Confirm that the information is correct for the Copy Pair that you have created 

Check the ‘Yes. I have …..’

Click on [Confirm] button to proceed to execute the pair creation. The configured task will be registered and executed based on the specified schedule.
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On the ‘Pair Configuration  ->Finish’ window

Click on [Finish] button to exit from Pair Configuration wizard

You can review  the Task completion status  under the ‘Task’ screen. 

3.0 Setting up  Replication (SI)
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From the HRpM screen

Click on the ‘Hosts’ panel. In the Hosts screen tick the Primary Volumes  (P-VOLs ) to be paired for Shadow Image  in the Paired view screen

Click on [Pair Management] button to launch the HRpM Pair Management Wizard

Click [Next] to continue to the PairAssociation screen
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In the copy topology screen , click on the LUN icon to the right of UR group as highlighted. This will pop- up another pair association group dialog

[image: image28.png]3 https:/ldnctisvhm001:23016 - Pair Configuration Wizard - Microsolt Internet Eplorer

1. Introduction b 2. Pair Association b 3. Group Management b 4. Task Management b 5. Confirm b 6. Finish

Add new pair group or modify existing pair group (copy roup). IF you want to save the settings as workflow, dick "Saue” bafore clicking "Cancel’

Copy Topology

Fdcacaatiadolp_18779_18350_02

£

uR

£

Dalare Group

Detail of Yolume

[ paruist | Valume selection
Filter By: Select Volume:
Valurne Tope: [prmary =] e [E
Resource: [ =] selection: [ 2]
Filer oy
Pairs: sie = |
Hostname: []
I~ Port/HSD/LUN & Subsystem Subsystem: -
I (Bott aioepsisdondon s v@ies106.152,145 (16950) P
I Dolie/deomatiadoic/0  USP V@165.166.192.144 (18850)
I DClie/rdeompatiadbic0C  USP V@165.166.152.144 (18850) Candidns
I DClie/rdeocpatiadbid/iD  USP V@165.166.152.144 (16850)
I DCLie/rdeompatiadbicl0E  USP_V@165.166.152.144 (16850)
I DClie/rdeompatiadoi/0r  USP_V@165.166.152.144 (18850)
I DClie/rdeompatiadbicrin  USP V@165.166.152.144 (16850)
I DClie/deomatiadoiril  USP V@165.166.152.144 (16850)
I Dclie/deomatiadoicriz  USP_V@165.166.192. 144 (16850) =(1]
< _ |
Fir [ o i w  — )
3 @ | . HMansge vour Ser... | (5 Ciprogram Fiest... | B CwinnTsyste... | B cawnTisyste... | 2 Caleulator | &7 Hiachi Device ... | &1 https:jfdnctisvh... [





Click on [Add Group] button to add new pair group for the selected  P-Vols .  This will bring up a ‘Add Pair Group’  dialog that will allow you to create  a new group into the topology at the top of the screen
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Enter a name for the new  pair group  following the recommended standards  (e.g  SI pairing <hostname>_<serailnum array>_SI

Select the copy Type for the new pair group. (eg SI for PIT copy)

Click the [OK] button to proceed
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The  Shadow Image Copy Group is added to the  original Copy Topology as highlighted.  We now need to set  up the Pair relationship
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On the Right –below  pane under  ‘Volume Selection’ ,start selecting the target Shadow Image volumes S-VOLs . Specify the filter conditions : Site (FDC or RDC), 

Host Name (Leave Blank), 

Subsystem ( Select remote ip & serial number)

Logical Group  . Click on the [Refresh ] button to start searching the voulmes that match the filter conditions.
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Select the Target volumes from the ‘Candidate’ list box

Click on [<Add Selection] button to add  selected volumes  as S-VOLs.
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Confirm the ‘Pair list’  listing for P=VOl and S-VOl association  is correct  and  click the [next] button
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On the ‘Group Management’ screen above 

Select the pair group that you want the copy group to be created. You will notice that the selected pair group is not assigned to any copy group.
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Click on [Create Group] button to create a copy group for the select ed pair group. This will pop up  a  ‘Create group’ dialog that will allow you to specify the pair managmenet servers and HORCM related parameters.
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On the ‘Create Group’ screen above

Confirm the Group Name has  the Copy  Group name entered earlier

Confirm the Primary and Secondary Pair Management server name . (They should be the same site  for Shadow Image)
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Specify the HORCM instance  number to create this Shadow Image copy Group ( Use the standards detailed in the check sheet 3 ->ShadowImage Primary     As these are already defined you will only need to select them from the drop down list.
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Specify the HORCM instance  number to create this Shadow Image copy Group ( Use the standards detailed in the check sheet 4 ->ShadowImage Secondary     As these are already defined you will only need to select them from the drop down list.

Click on [OK] button to proceed to create Copy Group
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On the ‘Group Management’ screen above.

The newly created copy group is shown on the left pane.

Click on [<Apply] button to add the copy pairs shown in the  ‘Pair  list’ Listing pane.
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On the ‘Task Management’ screen above , the list  of the tasks is displayed . One task  corresponds to one Copy Group.

Click [Next>] button to proceed to  the confirm window.
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On the ‘Pair Configuration->Confirm’ screens above

Confirm that the information is correct for the Copy Pair that you have created 

Check the ‘Yes. I have …..’

Click on [Confirm] button to proceed to execute the pair creation. The configured task will be registered and executed based on the specified schedule
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On the ‘Pair Configuration  ->Finish’ window

Click on [Finish] button to exit from Pair Configuration wizard

You can review  the Task completion status  under the ‘Task’ screen. 
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