
1.0 Software Tools Quick Reference
1.1 EMC
1.1.1 ViPR SRM (still in deployment/development phase)

Servers: Login using <soeid>/<local password>
http://nammsrmfe1.nam.nsroot.net:58080/APG/#
http://namusrmfe1.nam.nsroot.net:58080/APG/#

Sample of ViPR SRM main dashboard screen.
[image: ]




1.1.2 Unisphere for VMAX

Servers: Login using <soeid>/<AD soeid password>
390G – NAMEEMC01, 02
GTDC – NAMGEMC01, 02, 03
MWDC – NAMMEMC01, 02, 04, 05, 06, 07
O’Fallon – NAMMEMC03
Rutherford – NAMREMC01, 02
SWDC – NAMUEMC01, 02, 03, 04, 05, 06. 07
Jardines – LACPEMC01
[bookmark: _GoBack]QRDC – LACQEMC01

Default sceens setup for quick analysis…

Real time last hour (heatmap, IOPS, cache write pending, response time)
[image: ]

Diagnostic Last 24 Hours (heatmap, IOPS, cache write pending, response time)
[image: ]



Historical last 30 days (heatmap, cache write pending, front end port bust %, backend busy %)
[image: ]


1.1.3 Unisphere for VNX



1.2 HDS
1.2.1 Hitachi Command Suite (HCS)

Servers: Login using <soeid>/<AD soeid password>
390G – NAMEHDS03
GTDC – NAMGHDS03
MWDC – NAMMHDS03
Rutherford – NAMRHDS03
SWDC – NAMUHDS03

Sample HCS screenshot
[image: ]



1.3 IBM
1.3.1 IBM XiV GUI and TOP

Servers: Login using <soeid>/<AD soeid password>
MWDC – NAMMIBM01
SWDC – NAMUIBM01

Sample from XiV GUI statistics screen
[image: ]

Sample from XiV Top
[image: ]



1.4 Cisco
1.4.1 Data Center Network Manager (DCNM)

Servers: Login using <soeid>/<AD soeid password>
390G – NAMECISCOA02, B02
GTDC – NAMGCISCOA03, B03
MWDC – NAMMCISCOA03, B03
Rutherford – NAMRCISCOA02, B02
SWDC – NAMUCISCOA02, B02
Jardines – NAMMCISCOA04, B04
Monterrey – NAMGCISCOA04, B04
QRDC – LACQCISCOA01 B01

Sample DCNM Web Interface performace dashboard
[image: ]



Sample DCNM web interface end device performance detail
[image: ]



1.4.2 Cisco Fabric Manager and Device Manager

Sample DCNM Fabric Manager with Device Manager real-time summary screen open
[image: ]
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