[image: ]
Citi Technology Infrastructure	

EMEA SAN Storage Capacity Planning


	Day:
	Wednesday
	Date:
	21st  August 2013
	Time:
	11-12pm BST



	Participants

	Nigel Chilcott  (NC)
	
	Ashok Reddy (AR)
	

	
	
	
	






Figure 1 - EMC – VMAX and DMX Capacity
Pool Utilization 

	Site
	CGC
	CGC
	RDC
	RDC
	RDC
	RDC
	RDC
	RDC
	RDC
	RDC

	VMAX
	0623
	0745
	0552
	0678
	3286
	3073
	2230
	3696
	4330
	0347

	Enabled Pool Devices
	Total GB
	143393
	150517
	150517
	181999
	165454
	132133
	170969
	165454
	92412
	215267

	
	Used GB
	45746.5
	79203.3
	80684.9
	146273.5
	115836.9
	56759.1
	92658.3
	22900.3
	23639.4
	585.1

	
	% full
	31.90%
	52.62%
	53.61%
	80.37%
	70.01%
	42.96%
	54.20%
	13.84%
	25.58%
	0.27%

	Thin Devices
	# Devices
	5870
	3333
	3330
	9457
	8432
	15703
	7403
	9599
	4073
	6399

	
	Virtual Capacity GB
	197919
	112379
	112278
	318862
	284302
	529458
	249607
	323649
	137329
	215755

	
	capacity threshold
	164000
	109880
	109880
	328000
	330905
	264264
	242664
	328000
	328000
	328000

	
	# Allocated
	5469
	2771
	2802
	8270
	3899
	13589
	6246
	548
	1807
	344

	
	GB Allocated
	184398
	93430
	94475
	278840
	262925
	458180
	143162
	18477
	60927
	11599

	
	subscription
	128.60%
	62.07%
	62.77%
	153.21%
	158.91%
	346.76%
	83.74%
	11.17%
	65.93%
	5.39%

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	Site
	FDC
	FDC
	FDC
	FDC
	FDC
	FDC
	FDC
	ZDC
	ZDC
	

	VMAX
	0879
	3004
	2804
	2231
	3875
	4652
	0349
	2262
	0377
	

	Enabled Pool Devices
	Total GB
	193029
	132133
	82727
	275755
	82727
	188982
	215267
	55151
	33091
	

	
	Used GB
	158648.5
	59678.3
	59465.1
	167883.3
	11914.5
	40381.0
	33977.9
	11881.3
	5777.7
	

	
	% full
	82.19%
	45.17%
	71.88%
	60.88%
	14.40%
	21.37%
	15.78%
	21.54%
	17.46%
	

	Thin Devices
	# Devices
	9092
	12295
	4356
	10027
	4799
	7192
	6399
	2000
	1250
	

	
	Virtual Capacity GB
	306555
	414551
	146871
	338080
	161808
	242493
	215755
	67434
	42146
	

	
	capacity threshold
	328000
	264264
	328000
	352965
	328000
	328000
	328000
	110302
	66181
	

	
	# Allocated
	8164
	10725
	4046
	7555
	996
	1922
	2838
	1114
	523
	

	
	GB Allocated
	275266
	361615
	136419
	254732
	33582
	64804
	95689
	37561
	17634
	

	
	subscription
	142.60%
	273.68%
	164.90%
	92.38%
	40.59%
	34.29%
	44.45%
	68.11%
	53.29%
	

	
	
	
	
	
	
	
	
	
	
	
	



Figure 2 - HDS – USP-V and VSP’s– Capacity:
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	Site
	Riverdale DC
	Riverdale DC
	Riverdale DC
	Frankfurt DC
	Frankfurt DC
	

	Array Alias
	RDCHDS02
	FDCHDS02
	

	Serial #
	18850
	18850
	18850
	18779
	18779
	

	PoolID
	1
	2
	22
	1
	2
	

	Tier
	3
	4
	4
	3
	4
	

	Enabled Pool Devices
	Total GB
	12,184
	20,667
	61,536
	12,184
	82,668
	

	
	Used GB
	4,043.4
	17,154.3
	20,610.9
	4,472.9
	73,863.4
	

	
	% full
	33.19%
	83.00%
	33.49%
	36.71%
	89.35%
	

	Thin Devices
	# Devices
	681
	1,076
	1,992
	681
	2,660
	

	
	Virtual Capacity GB
	22,474
	43,115
	90,004
	22,474
	122,051
	

	
	Threshold capacity
	24,368
	41,334
	56,582
	24,368
	121,652
	

	
	# Allocated (Est)
	350
	716
	1,456
	384
	2,338
	

	
	GB Allocated
	10,997
	30,618
	35,662
	12,184
	110,887
	

	
	subscription
	90.26%
	148.15%
	57.95%
	100.00%
	134.13%
	

	
	
	
	
	
	
	
	

	Site
	Riverdale DC
	Riverdale DC
	Frankfurt DC
	Frankfurt DC
	Frankfurt DC
	

	Array Alias
	RDCHDS03
	FDCHDS03
	

	Serial #
	78378
	78378
	78398
	78398
	78398
	

	PoolID
	1
	2
	1
	2
	22
	

	Tier
	3
	4
	3
	4
	4
	

	Enabled Pool Devices
	Total GB
	31,940
	15,031
	31,940
	37,577
	39,390
	

	
	Used GB
	6,365.7
	8,337.6
	7,093.7
	13,498.7
	13,455.7
	

	
	% full
	19.93%
	55.47%
	22.21%
	35.92%
	34.16%
	

	Thin Devices
	# Devices
	1,439
	901
	1,462
	1,630
	1,354
	

	
	Virtual Capacity GB
	48,095
	31,256
	47,312
	64,316
	66,712
	

	
	Threshold capacity
	46,507
	30,141
	46,507
	75,153
	56,249
	

	
	# Allocated (Est)
	376
	340
	444
	468
	926
	

	
	GB Allocated
	11,226
	11,795
	12,007
	24,006
	17,449
	

	
	subscription
	35.15%
	78.47%
	37.59%
	63.88%
	44.30%
	

	
	
	
	
	
	
	
	

	Site
	Riverdale DC
	Frankfurt DC
	Frankfurt DC
	Riverdale DC
	Riverdale DC
	Riverdale DC

	Array Alias
	RDCHDS04
	DEOLH005N0365
	DEOLH004N7026
	GBOKH005N3518
	GBOKH006N5362

	Serial #
	78998
	90365
	97026
	53518
	53518
	55362

	PoolID
	20
	20
	20
	20
	50
	20

	Tier
	4
	4
	4
	4
	4
	4

	Enabled Pool Devices
	Total GB
	142,778
	202,908
	210,428
	172,852
	76,591
	172,852

	
	Used GB
	82,844.5
	110,400.4
	40,137.0
	13,592.9
	33,968.0
	75,320.8

	
	% full
	58.02%
	54.41%
	19.07%
	7.86%
	44.35%
	43.58%

	Thin Devices
	# Devices
	3,896
	1,630
	1,354
	681
	1,076
	1,992

	
	Virtual Capacity GB
	130,640
	64,316
	66,712
	22,474
	43,115
	90,004

	
	Threshold capacity
	213,518
	75,153
	56,249
	345,703
	153,182
	56,582

	
	# Allocated (Est)
	3,310
	5,086
	926
	2,828
	1,015
	1,456

	
	GB Allocated
	93,146
	184,194
	268,560
	96,956
	41,000
	179,246

	
	subscription
	65.24%
	90.78%
	127.63%
	56.09%
	53.53%
	103.70%





Figure 3 – EMC - Clariion Capacity:

	Site
	Array
	Alias
	Total Raw Capacity (TB)
	Free Raw Capacity (TB)
	Total Usable Capacity(TB)
	Free Capacity (TB)

	Riverdale DC
	CKM00091100696
	rdc4-cx4-0696
	131.79
	0.73
	83.43
	0.45

	
	CKM00101000576
	rdc4-ac4-0576
	44.02
	25.48
	22.52
	12.74

	
	FCNMM092500021
	rdc1-ax4-0021
	8.22
	0.80
	4.31
	0.40

	
	FCNMM092500023
	rdc1-ax4-0023
	8.22
	0.80
	4.31
	0.40

	
	FCNMM092500024
	rdc1-ax4-0024
	8.22
	0.80
	4.31
	0.40

	
	FCNMM092500026
	rdc1-ax4-0026
	8.22
	1.19
	4.31
	0.79

	
	FCNMM092500033
	rdc1-ax4-0033
	8.22
	0.80
	4.31
	0.40

	
	FCNMM092500034
	rdc1-ax4-0034
	8.22
	0.80
	4.31
	0.40

	
	FCNMM092500040
	rdc1-ax4-0040
	8.22
	0.80
	4.31
	0.40

	
	FCNMM092500042
	rdc1-ax4-0042
	8.22
	0.80
	4.31
	0.40

	
	FCNMM111600082
	rdc1-ax4-0082
	5.50
	1.88
	2.88
	0.94

	
	SL7EA102100006
	rdc4-ax4-0006
	10.73
	3.75
	5.50
	1.88

	
	SL7EA102100007
	rdc4-ax4-0007
	10.73
	3.75
	5.50
	1.88

	Frankfurt DC
	FCNMM092200023
	fdc1a-ax4-0023
	8.22
	0.80
	4.31
	0.40

	
	FCNMM111100069
	fdc1a-ax4-0069
	5.50
	1.88
	2.88
	0.94

	
	SL7E1090800045
	fdc1a-ax4-0045
	8.22
	0.80
	4.31
	0.40

	
	SL7E1090800055
	fdc1a-ax4-0055
	8.22
	0.80
	4.31
	0.40

	
	SL7E1091600092
	fdc1a-ax4-0092
	8.22
	0.80
	4.31
	0.40

	
	SL7E1091700038
	fdc1a-ax4-0038
	8.22
	0.80
	4.31
	0.40

	
	SL7E1091900060
	fdc1a-ax4-0060
	8.22
	0.80
	4.31
	0.40

	
	SL7E1091900096
	fdc1a-ax4-0096
	8.22
	0.80
	4.31
	0.40

	
	SL7E1091900118
	fdc1a-ax4-0118
	7.96
	0.80
	4.05
	0.40

	
	SL7EA101700033
	fdc1a-ax4-0033
	10.73
	3.75
	5.50
	1.88

	
	SL7EA101700039
	fdc1a-ax4-0039
	10.73
	3.75
	5.50
	1.88

	Turkey DC
	SL7E1093200048
	Turkey_AX4
	4.44
	0.53
	2.48
	0.33

	Russia DC
	SL7E9101300054
	prof-ax4-0054
	14.40
	0.00
	10.47
	0.00

	
	SL7E9101300062
	pres-ax4-0062
	14.53
	0.00
	10.60
	0.00

	
	FCNMM113000127
	prof-ax4-0127
	8.25
	0.00
	4.32
	0.00

	 
	 
	Total
	402.66
	58.63
	230.23
	29.66




Figure 4 – EMC - Centera Capacity:

	Country
	Type
	Array
	Approx number of weeks Available
	Total Storage on Centera - (Available + Used Capacity)
	% Available
	Used Capacity 
	Available Space

	Poland
	Voice
	PL_01G CK200053810059
	35.75
	57124
	15.07
	48517
	8607

	
	 
	Used per Week
	 
	 
	 
	 
	84

	
	Voice
	PL_01S CK200054900293
	90.9
	77266
	34.18
	50856
	26410

	
	 
	Used per Week
	 
	 
	 
	 
	53

	
	AXSPnt
	PL_02G CK200042100431
	207.88
	40003
	63.63
	14549
	25454

	
	 
	Used per Week
	 
	 
	 
	 
	20

	
	AXSPnt
	PL_02S CK200042100432
	182.65
	40002
	63.63
	14547
	25455

	
	 
	Used per Week
	 
	 
	 
	 
	21

	Switzerland
	Voice
	CH_01E CK200053010120
	52.3
	46080
	71.11
	13312
	32768

	
	 
	Used per Week
	 
	 
	 
	 
	0

	
	Voice
	CH_01R CK200054900163
	242.82
	
	
	.
	28672

	
	 
	Used per Week
	 
	 
	 
	 
	0

	Turkey
	Voice
	TK_01T CK200054900292
	5.07
	50509
	6.31
	47323
	3186

	
	 
	Used per Week
	 
	 
	 
	 
	2601

	
	Voice
	TK_01Y CK200054900294
	28.66
	49835
	18.12
	40806
	9029

	
	 
	Used per Week
	 
	 
	 
	 
	83

	UK/DE
	Voice
	UK_01R CK200061900567
	58.52
	245070
	37.15
	154031
	91039

	
	 
	Used per Week
	 
	 
	 
	 
	378

	
	Voice
	DE_01E CK200061900265
	59.7
	248112
	37.89
	154094
	94018

	
	 
	Used per Week
	 
	 
	 
	 
	478

	
	Voice
	DE_02E CK200062000592
	75.51
	99475
	27.69
	71935
	27540

	
	 
	Used per Week
	 
	 
	 
	 
	0

	
	Voice
	UK_02R CK200062000593
	91.95
	105496
	29.35
	74530
	30966

	
	 
	Used per Week
	 
	 
	 
	 
	-271

	RDC/FDC
	CEEMEA
	rdccentera01 CK200113804158
	304.47
	25595
	83.86
	4130
	21465

	
	 
	Used per Week
	 
	 
	 
	 
	28

	
	CEEMEA
	fdccentera01 CK200113804159
	123.24
	25604
	67.92
	8214
	17390

	
	 
	Used per Week
	 
	 
	 
	 
	55




Figure 5 – Switch Utilisation and Capacity:



	DC
	Switches Type
	Switches: # Fabrics
	Switches: # Switch Ports
	Switches: # Free Ports
	Switches: # ISL Ports
	Switches: # Ports to Hosts/HBAs
	Switches: # Ports to Storage
	Switches: # Ports to Unidentified
	Total ports Used

	FDC
	McDATA
	0
	0
	0
	0
	0
	0
	0
	0

	[image: https://ukctiprsa38.eur.nsroot.net:30002/srm/img/ascending.gif]
	RDC



	McDATA
	29
	3279
	1416
	318
	782
	129
	634
	1863

	CGC
	McDATA
	19
	1856
	464
	216
	271
	32
	873
	1392

	 
	 
	48
	5135
	1880
	534
	1053
	161
	1507
	3255





	DC
	Switches Type
	Switches: # Fabrics
	Switches: # Switch Ports
	Switches: # Free Ports
	Switches: # ISL Ports
	Switches: # Ports to Hosts/HBAs
	Switches: # Ports to Storage
	Switches: # Ports to Unidentified
	Total ports Used

	FDC
	Cisco
	95
	4188
	1460
	350
	1417
	444
	517
	2728

	RDC
	Cisco
	85
	5076
	1818
	388
	1793
	431
	646
	3258

	CGC
	Cisco
	37
	3432
	1778
	118
	200
	39
	1297
	1654

	 
	 
	217
	12696
	5056
	856
	3410
	914
	2460
	7640

















Figure 6 – EMC/HDS - Tech Refresh 

Below full list of all EOL source arrays

	Location
	Frame
	Serial number
	Vendor
	Storage Tier
	Replication Partner
	Model

	RDC
	Sym-290102819
	290102819
	EMC
	Non-Rep
	 
	Symmetrix DMX3-24

	RDC
	Sym-290102839
	290102839
	EMC
	Replicated
	Sym-290102838
	Symmetrix DMX3-24

	CGC
	Sym-290102838
	290102838
	EMC
	Replicated
	Sym-290102839
	Symmetrix DMX3-24

	CGC
	Sym-290101868
	290101868
	EMC
	Non-Rep
	 
	Symmetrix DMX3-24

	FDC
	fdchds02_18779 - Thin
	18779
	HDS
	Replicated
	RDCHDS02 - Thin
	R600

	FDC
	fdchds02_18779 - Thin
	
	HDS
	Non-Rep
	 
	R600

	RDC
	RDCHDS02
	18850
	HDS
	Non-Rep
	 
	R600

	RDC
	RDCHDS02 - Thin
	
	HDS
	Replicated
	fdchds02_18779 - Thin
	R600

	RDC
	RDCHDS02 - Thin
	
	HDS
	Non-Rep
	 
	R600

	FDC
	Sym-290103943
	290103943
	EMC
	Non-Rep
	 
	Symmetrix DMX4-24

	CGC
	Sym-290103336
	290103336
	EMC
	Replicated
	Sym-290103471
	Symmetrix DMX4-24

	FDC
	Sym-290103810
	290103810
	EMC
	Replicated
	Sym-290103720
	Symmetrix DMX4-24

	RDC
	Sym-290103720
	290103720
	EMC
	Replicated
	Sym-290103810
	Symmetrix DMX4-24

	FDC
	Sym-290103564
	290103564
	EMC
	Non-Rep
	 
	Symmetrix DMX4-24

	FDC
	Sym-290103550
	290103550
	EMC
	Replicated
	Sym-290103471
	Symmetrix DMX4-24

	RDC
	Sym-290103471
	290103471
	EMC
	Replicated
	Sym-290103550
	Symmetrix DMX4-24

	FDC
	Sym-290103544
	290103544
	EMC
	Replicated
	Sym-290103452
	Symmetrix DMX4-24

	RDC
	Sym-290103452
	290103452
	EMC
	Replicated
	Sym-290103544
	Symmetrix DMX4-24

	RDC
	Sym-290103452
	
	EMC
	Non-Rep
	 
	Symmetrix DMX4-24

	RDC
	RDCHDS01
	75189
	HDS
	Non-Rep
	 
	R600







Below are Target arrays

	To either non-replicated HDS Arrays:

	1. RDC GBOKH006N5362 (BAU-TR VSP)

	2. FDC DEOLH005N0365 (BAU-TR VSP)

	

	or Replicated EMC Arrays:

	3. RDC Rep 000292604330 (EMC VMAX)

	4. FDC Rep 000292604652 (EMC VMAX)

	

	Or new Non-rep EMC arrays:

	5. RDC non-rep CK295700347 (EMC VMAX)

	6. FDC non-rep CK295700349 (EMC VMAX)

	




Project Objective
The migration of data from 16 older frames to EMC/HDS Storage Arrays:
•             Total Frames: 18 (including HDS03 transferred from Smart421)
•             Total Servers: 1376
•             Thick to Thin 

Current Status
· 40 hosts migrated this week
· Citi to make decision on the cost options of migrating hosts that are connected to the McData Fabric (93 hosts) 
· STAR replication hosts on hold until agreement is reached with the business (30 hosts)

Issues
· 24x hosts postponed by the SA due to lack of approval from the business

Activities planned for next 1-3 weeks
· 50 hosts planned for the 3rd of July.

Summary of Migration Progress
	Scope
	 

	Total Number of Servers
	1376

	Servers to be, assumed or decommissioned
	87

	Hosts connected to McData
	93

	Total Number of Servers To Be Migrated
	767

	Number of Servers Migrated
	429
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=================

As discussed last week, we are fairly closed to using up all the allocated capacities on the HDS arrays in FDC. As agreed, as part of the TR project we will therefore be over allocating to 125% of the actual capacity. This you have advised is and always been the policy in EMEA.

Please let me know if you need to add anything further or provide any further clarification.

Below are the capacity figures promised, will provide 3518 figures as soon as updated figures are available.

Regards,
Nik Doshi


FDC VSP_7026
Actual: 205 TB
Configured: 316 TB
Actual Allocated: 262 TB
Actual Used: 39 TB (19%)

FDC VSP_0365
Actual: 198 TB
Configured: 234 TB
Actual Allocated: 179 TB
Actual Used: 112 TB (56%)

RDC VSP_5362
Actual: 168 TB
Configured: 227 TB
Actual Allocated: 175 TB
Actual Used: 74 TB (44%)

RDC VSP_3518 (not the latest figures, awaiting update)
Actual: 243 TB
Configured: 312 TB
Actual Allocated: 102 TB
Actual Used: 40 TB


==========================

0365 in FDC is only 90% allocated but is already 56% utilised. This is far higher utilisation than all other arrays. Would we still allocate 125% on this array?

If not, I think we are 20TB’s away from hitting capacity constrains in FDC (non-rep) as 7026 is already 125% utilised.











Figure 7 - “Archive” storage (KDB use only):

	Description
	Configuration
	Usable 
	Type
	S.No
	 
	Application
	Used (TB)
	Available (TB)

	RDC Archive
	32 x 3TB
	73.63
	VSP upgrade
	53518
	 
	KDBRDC
	40
	33.63

	CGC Equities
	32 x 3TB
	73.63
	HUS-VM
	10214
	 
	KDBCGC
	40
	33.63





Figure 8 - “Bronze” Storage:

	Description
	Configuration
	Usable 
	Type
	S.No
	 
	Application
	Used (TB)
	Available (TB)

	RDC Non-Rep Bronze
	96 x 600GB
	43.37
	HUS-VM
	10204
	 
	 
	0
	43.37

	FDC Non-Rep Bronze
	96 x 600
	44
	HUS-VM
	10516
	 
	 
	0
	44





Rainbow Project :-

· Poland cut-over is on 21st July 2013 and they are requesting buffer capacity of 2TB on emergency purpose

· Rainbow Project requirements - Rainbow PM confirmed by below forecast capacity for 2013 
· Leg1 28tb
· Leg2 15tb
· Non rep – RDC 18tb
· FDC 0tb
In summary:

Leg 1:
· CK292602804 – FDC  – Current capacity 82.6TB usable
Convert to RAID1 and increase (add new disks) usable capacity to 113.2TB – net 30.9TB usable increase 
Cost to Citi - $480,906

· CK292603286 – RDC – Current capacity 165.29TB usable
Convert to RAID1 and increase (add new disks) usable capacity to 226.4TB – net 61.11TB usable increase 
Cost to Citi - $933,129

Leg 2:
· CK292603875 – FDC – Current capacity 82.6TB usable
Convert to RAID1 and increase (add new disks) usable capacity to 88TB – net 5.4TB usable increase 
Cost to Citi - $324,419

· CK292603696 – RDC – Current capacity 165.29TB usable
Convert to RAID1 and increase (add new disks) usable capacity to 186.67TB – net  21.38TB usable increase 
Cost to Citi - $428,490

EMC services to assure successful RAID migrations
Cost to Citi - $166,414

Total Cost to Citi:  $2,333,358

Note – Alternative option considered was to refresh all 4 arrays (Leg1/Leg2) to EMC VMAX40K – the cost of this option was greater than 3 times the cost of the upgrading the current array to RAID1.  Conversion from RAID6 protection level to RAID1 - on the Backend of all Rainbow arrays (both Leg 1 and 2) – will bring the arrays in line with new CATE standard for Replicated arrays.   


Announcements / Recent Issues
· Tier 4 allocations on V-Max 3073 & 3004 are now subject to the same allocations restrictions as V-Max 0678 & 0879 – i.e. 
· V-Max 3073 & 3004 – No NEW allocations, growth of existing data-sets only.
All NEW allocations to be reserved on VSP (restrictions apply)

· More guidelines (restrictions?) have been imposed upon Storage allocations
· All new replicated requests will be allocated on EMC only (no other option available).
· Clustered datasets will be allocated as follows:
· Single dataset on replicated clusters will be allocated on a single EMC array 
· Single dataset on non-replicated clusters will be allocated on an HDS or EMC single array.
· Two or more separate data sets on non-replicated clusters can be allocated on both, provided every dataset is kept to one vendor.
· A host that has been allocated non-replicated HDS and replicated EMC is certified. 
· A multi-host environment that has been allocated PROD/COB on EMC and DEV/UAT on HDS is certified.
· Any host supporting cloning (i.e. Flexcube) will be allocated on EMC only.
· CITISWITCH. Prod, COB, UAT and Development will be allocated on EMC only (SM directive).
· VMware – all new T4 to be allocated on HDS wherever possible
· 4 FA ports to be used for all VMAX allocations

Please note: The above guidelines apply to SILVER storage ONLY.  There are currently no specific guidelines for GOLD, BRONZE or ARCHIVAL storage.


Action Items:

As per Figure 1 -– What to do with the highlighted in red / yellow? Move hosts to other arrays. Which hosts? What is the impact?

· Frame 678 – Pool Utilization is ~80% and over subscription is 152%
· Frame 879 - Pool Utilization is ~85% and over subscription is 142%
· Frame 3073 - Pool Utilization is ~45% and over subscription is 350%
· Frame 3004 - Pool Utilization is ~43% and over subscription is 285%
· Frame 2804 - Pool Utilization is ~69% and over subscription is 164%
· Frame 3286 - Pool Utilization is ~67% and over subscription is 158%

· For 678 , 879, 3073 & 3004 – Action Plan
· identify Unused devices and perform reclaims 
· Need to move some of the hosts to other newly installed frames
· Recommends to raise a separate project and migrate the hosts to other Array

· For 2804 & 3286 – Action Plan
· Rainbow PM confirmed there is no reclaims on Leg1 frmae
· Rainbow team is planning to move some of hosts from Leg1 to Leg2 frame
		

Bronze Storage:  To be offered to  “Tech refresh” and “new allocation” customers only
· Rate Card needs updating include this type of storage.
· TCRS needs updating 
· A document – compiled by SAN team – will be created to make potential customers aware of the differences in storage performance & capabilities between so-called “non-Replicated” and “Bronze”
[bookmark: _GoBack]
McData Migration:

The following arrays are attached to the McData fabric in RDC.

· RDCHDS01
· RDCVMAX01
· RDCHDS04
· DMX SYMM21R
· DMX SYMM22R
· GBOKH005N3518-(rdchds05) – used for migrations
· GBOKH006N5362-(rdchds06) – used for migrations

Reports:-

Host Billing Report : Completed

MOR Report : Completed

New Installations / Decommissions  / Physical Location Limitations




AOB & Updates:

· If the pool utilization is more than 70% then mark as RED
· If over-subscription is between 130% to 150% then mark as Amber
· If over-subscription is more than 150% then mark as RED
· There is no way we can add additional drives on frame #678. So need to perform reclaims or migrate the disks to new frames
·  Need to run ZSR on BCVs to reduce the pool utilization on Rainbow COB frame # 3286
· Move the High I/O LUNs  to SATA disks are not recommended as per the CATE as it is a non-standard on EMEA Rainbow frame#2804
· Need to amend the installed capacity on #347 as it is showing wrongly
· Had a discussion to include vnx arrays info
· Clariion capacity is not required to display as it is not going increase
· Bronze rate card is not ready

	Date
	Task
	Assigned To
	Status

	21/08/2013
	Bronze storage documentation
	Krishnam/Nigel
	

	21/08/2013
	Archival storage capacity need to update
	Ashok
	

	21/08/2013
	Turkey centera capacity issue
	Ashok/Sal
	

	21/08/2013
	update the No of weeks available - Centera capacity
	Ashok
	

	21/08/2013
	Tech refresh migration status
	Ashok/Nick
	

	21/08/2013
	678 , 879, 3073 & 3004–plan of action to release/migrate the disks to new frames
	Ashok/Sal
	

	
	
	
	

	
	
	
	

	
	
	
	







	Next Meeting:

	Day:
	Friday
	Date:
	30th August 2013
	Time:
	11:00 – 12:00hrs GMT
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