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	Objective
Objective
	HDS Provisioning Steps

	Date
	04/07/2006
	Telephone Bridge:
	(866) 445-7018
	Pass Code:
	147857

	Frequency
	Weekly
	Facilitator:   
	Scott Higgins
	
	

	Start
	03:00 PM ET
	Stop Time:
	
	Total Hours: 
	

	

	Attended By:

	Jeff Taylor, Gerry Cruz, Doug Novellano, Raja Balasubramanian, Kranthi Tummala. 

	

	References:

	


	
	Meeting Agenda Items 
	Speaker 
	Comments

	1. 
	Host Groups - timing of this change.
	
	Storage is that allocated to a specific server.  It includes a server WW address, port number, storage devices.  In terms of EMC, it would equate to a symconfigure and mapping devices to an FA.  Varying opinions in regards to this as to what the true impact is.  EMC symconfigure – you are updating all FA’s, no safeguards.  

HDS – not updating all CHA’s, there are safeguards in place.  

If you take a device in an existing storage group and move it, you can cause a serious issue.   There are no warning messages in regards this.  

The consensus is that this is equivalent to a VCM update. 

The team consensus is that these changes will be done after hours.  

	2. 
	LUN Numbering
	
	The issue is whether we predefine LUN numbers or pick them on the fly. 

Jeff – Predefine

Raja – use incremental LUN numbers as we go along. 

There were some varying opinions and the team would like to discuss this again.  Scott Higgins to setup a follow-up next Wed. 



	
	Device Sizes
	
	Not discussed. 

	3. 
	Pre-configuring LUNS vs. Non-Preconfiguration.
	
	The decision is the pre-configure – this was a management decision - Scott Higgins to verify.  

	4. 
	
	
	


	Meeting Notes

	Open Discussion:
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