Step1 : - 

1) Run Below command in cgcsan-mgt1

for i in `symdg list -v | grep "Group Name:"|awk '{print $3}'`;do symrdf -g $i verify -synchronized|grep None;done
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2) Run Below command in fdcsan-mgt1 & fdcctisanla01p

for i in `symdg list -v | grep "Group Name:"|awk '{print $3}'`;do symrdf -g $i verify -consistent|grep None;done
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3) Run Below command in fdcsan-mgt1 & rdcsan-mgt1

for i in `cat /etc/horcm0.conf|grep 9901|awk '{print $1}'`;do perl  /var/opt/san/scripts/HDS/bin/HUR_2DC_display -g $i|grep PSUS;done
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Step2 : - 

The above commands will generate below output
None of the devices in the group 'fdcgcgcpldbc01p_2p_2804_A115' are in 'Consistent' state.

Device group 'gtsncsap11p_12p_3452_3544_A41' is invalid.
So please note down replication group name and  run the below command on san management stations to get the status of the replication group.
Symrdf –g fdcgcgcpldbc01p_2p_2804_A115 query 
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Step3 : - 
Please open the excel sheet and note down the status of the SAN replication group like below format

	S.No
	SAN MGMT
	Replication Group
	Status

	1
	fgcctisanla01p
	fdcgcgcpldbc01p_2p_2804_A115
	ACP_Disk Mode

	2
	fgcctisanla01p
	fdcgcgdbcsd01p_2p_2804_3286_A85
	ACP_Disk Mode

	3
	fgcctisanla01p
	rdcgtsefywd01p_2230_2231_A65
	SPLIT State

	4
	fdcsan-mgt1
	eba2_3452_3544_A
	SPLIT State

	5
	fdcsan-mgt1
	gtsmigad_temp
	SPLIT State

	6
	fdcsan-mgt1
	rdcgtsrbwwd01p_3720_3810_A13
	Suspended

	7
	cgcsan-mgt1
	eqdbcgc3_4p_0745_0552
	invalid

	8
	cgcsan-mgt1
	eqemsap7_8p_0745_0552
	Failed Over

	9
	cgcsan-mgt1
	eqexch5_6_7_8p_0745_0552
	SPLIT State

	10
	RDC-HDS
	RDCGCTGFTWA01P_78378_78398_0D
	SPLIT State

	11
	RDC-HDS
	rdcgcgemvwa01p_78378_78398_3D
	SPLIT State

	12
	FDC-HDS
	fdcgcggenaa01p_18779_18850_18
	SPLIT State

	13
	FDC-HDS
	fdcgcggenad01_2p_18779_18850_1A
	SPLIT State


